(export (version D)
  (design
    (source /data/Git/IOT/LORA_ATTINY84/LORA_ATTINY84.sch)
    (date "Mi 28 Aug 2019 10:33:34 CEST")
    (tool "Eeschema 5.1.4")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source LORA_ATTINY84.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value ATtiny84A-SSU)
      (footprint Package_SO:SOIC-14_3.9x8.7mm_P1.27mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf)
      (libsource (lib MCU_Microchip_ATtiny) (part ATtiny84A-SSU) (description "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-14"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D66342E))
    (comp (ref J1)
      (value Sensor)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x08_Male) (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D68DC89))
    (comp (ref AE1)
      (value Antenna)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part Antenna) (description Antenna))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D699DFD))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B1612))
    (comp (ref C1)
      (value 100n)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6B2940))
    (comp (ref J2)
      (value PRG)
      (footprint Connector_PinSocket_2.54mm:PinSocket_2x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x03_Odd_Even) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D69C5BF))
    (comp (ref BT1)
      (value Battery_Cell)
      (footprint Battery:BatteryHolder_Keystone_1060_1x2032)
      (datasheet ~)
      (libsource (lib Device) (part Battery_Cell) (description "Single-cell battery"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6F40EE))
    (comp (ref U2)
      (value RFM95W-868S2)
      (footprint RFM9X:RFM9X-TH)
      (datasheet https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)
      (libsource (lib RF_Module) (part RFM95W-868S2) (description "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwith 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D664943)))
  (libparts
    (libpart (lib Connector) (part Conn_01x08_Male)
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x03_Odd_Even)
      (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x03_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Device) (part Antenna)
      (description Antenna)
      (docs ~)
      (fields
        (field (name Reference) AE)
        (field (name Value) Antenna))
      (pins
        (pin (num 1) (name A) (type input))))
    (libpart (lib Device) (part Battery_Cell)
      (description "Single-cell battery")
      (docs ~)
      (fields
        (field (name Reference) BT)
        (field (name Value) Battery_Cell))
      (pins
        (pin (num 1) (name +) (type passive))
        (pin (num 2) (name -) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_Microchip_ATtiny) (part ATtiny24V-10SSU)
      (aliases
        (alias ATtiny24-20SSU)
        (alias ATtiny24A-SSU)
        (alias ATtiny44V-10SSU)
        (alias ATtiny44-20SSU)
        (alias ATtiny44A-SSU)
        (alias ATtiny84V-10SSU)
        (alias ATtiny84-20SSU)
        (alias ATtiny84A-SSU))
      (description "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-14")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf)
      (footprints
        (fp SOIC*3.9x8.7mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATtiny24V-10SSU)
        (field (name Footprint) Package_SO:SOIC-14_3.9x8.7mm_P1.27mm))
      (pins
        (pin (num 1) (name VCC) (type power_in))
        (pin (num 2) (name XTAL1/PB0) (type 3state))
        (pin (num 3) (name XTAL2/PB1) (type 3state))
        (pin (num 4) (name ~RESET~/PB3) (type 3state))
        (pin (num 5) (name PB2) (type 3state))
        (pin (num 6) (name PA7) (type 3state))
        (pin (num 7) (name PA6) (type 3state))
        (pin (num 8) (name PA5) (type 3state))
        (pin (num 9) (name PA4) (type 3state))
        (pin (num 10) (name PA3) (type 3state))
        (pin (num 11) (name PA2) (type 3state))
        (pin (num 12) (name PA1) (type 3state))
        (pin (num 13) (name AREF/PA0) (type 3state))
        (pin (num 14) (name GND) (type power_in))))
    (libpart (lib RF_Module) (part RFM95W-868S2)
      (aliases
        (alias RFM95W-915S2)
        (alias RFM96W-315S2)
        (alias RFM96W-433S2)
        (alias RFM97W-868S2)
        (alias RFM97W-915S2)
        (alias RFM98W-315S2)
        (alias RFM98W-433S2)
        (alias RFM69HCW))
      (description "Low power long range transceiver module, SPI and parallel interface, 868 MHz, spreading factor 6 to12, bandwith 7.8 to 500kHz, -111 to -148 dBm, SMD-16, DIP-16")
      (docs https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)
      (footprints
        (fp HOPERF*RFM9XW*))
      (fields
        (field (name Reference) U)
        (field (name Value) RFM95W-868S2))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name MISO) (type output))
        (pin (num 3) (name MOSI) (type input))
        (pin (num 4) (name SCK) (type input))
        (pin (num 5) (name NSS) (type input))
        (pin (num 6) (name RESET) (type BiDi))
        (pin (num 7) (name DIO5) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name ANT) (type BiDi))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name DIO3) (type BiDi))
        (pin (num 12) (name DIO4) (type BiDi))
        (pin (num 13) (name 3.3V) (type power_in))
        (pin (num 14) (name DIO0) (type BiDi))
        (pin (num 15) (name DIO1) (type BiDi))
        (pin (num 16) (name DIO2) (type BiDi)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical MCU_Microchip_ATtiny)
      (uri /usr/share/kicad/library/MCU_Microchip_ATtiny.lib))
    (library (logical RF_Module)
      (uri /usr/share/kicad/library/RF_Module.lib)))
  (nets
    (net (code 1) (name +3V3)
      (node (ref J1) (pin 8))
      (node (ref BT1) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 13)))
    (net (code 2) (name GND)
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 10))
      (node (ref J1) (pin 7))
      (node (ref BT1) (pin 2))
      (node (ref C1) (pin 1))
      (node (ref J2) (pin 6))
      (node (ref C2) (pin 2))
      (node (ref U1) (pin 14))
      (node (ref U2) (pin 8)))
    (net (code 3) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 4) (name DIO0)
      (node (ref U1) (pin 2))
      (node (ref U2) (pin 14)))
    (net (code 5) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 6) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 7) (name NSS)
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 3)))
    (net (code 8) (name "Net-(U2-Pad6)")
      (node (ref U2) (pin 6)))
    (net (code 9) (name "Net-(AE1-Pad1)")
      (node (ref AE1) (pin 1))
      (node (ref U2) (pin 9)))
    (net (code 10) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 11) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 12) (name PA3)
      (node (ref U1) (pin 10))
      (node (ref J1) (pin 3)))
    (net (code 13) (name PA2)
      (node (ref U1) (pin 11))
      (node (ref J1) (pin 4)))
    (net (code 14) (name PA1)
      (node (ref U1) (pin 12))
      (node (ref J1) (pin 5)))
    (net (code 15) (name PA0)
      (node (ref U1) (pin 13))
      (node (ref J1) (pin 6)))
    (net (code 16) (name PB2)
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 17) (name PA7)
      (node (ref U1) (pin 6))
      (node (ref J1) (pin 2)))
    (net (code 19) (name MISO)
      (node (ref J2) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U2) (pin 2)))
    (net (code 20) (name SCK)
      (node (ref J2) (pin 3))
      (node (ref U1) (pin 9))
      (node (ref U2) (pin 4)))
    (net (code 21) (name MOSI)
      (node (ref U1) (pin 7))
      (node (ref J2) (pin 4))
      (node (ref U2) (pin 3)))
    (net (code 22) (name RST)
      (node (ref J2) (pin 5))
      (node (ref U1) (pin 4)))))